FORM Spec BDS, Revised 02/05 	COPYRIGHT © 2005 SHIPPENSBURG PUMP COMPANY, INC. 
Shipco® IS A REGISTERED TRADEMARK OF SHIPPENSBURG PUMP CO., INC. 	PRINTED IN THE U.S.A. • BEIDEL PRINTING HOUSE, INC., 717-532-5063
SHIPPENSBURG PUMP COMPANY, INC., P.O. BOX 279, SHIPPENSBURG, PA 17257
PHONE 717-532-7321 • FAX 717-532-7704 • www.shipcopumps.com
_______________________________________________________________________________________
SUGGESTED SPECIFICATIONS	SHIPCO® PUMPS
TYPE BDS BlowDown Separator
CAPACITY SCHEDULE MUST BE COMPLETED.
Furnish and install according to drawings and manufacturer’s instructions the quantity of BDS blowdown separators as shown on the drawings. Each unit shall consist of (1) ASME code stamped steel receiver, with automatic after section and inlet, vent and drain tappings as indicated below.
The blowdown tank shall be manufactured of steel ASME code stamped. The receiver shall be elevated with stand and equipped with: stainless steel wear plate, tangential inlet tapping and an automatic aftercooler section with automatic discharge temperature regulating valve, gate valve, wye strainer and thermometer. The receiver tank size shall be as shown on the drawings.
The unit shall be factory tested as a complete unit. The pump manufacturer shall furnish complete elementary connection and piping diagrams.
Manufacturer shall be Shipco® PUMPS, P.O. Box 279, Shippensburg, PA 17257.
Capacity Schedule (Required to complete suggested specifications).
TYPE BDS BLOWDOWN SEPARATOR SCHEDULE:
Catalog No. __________ BDS
INLET __________ "
VENT __________ "
DRAIN __________ "
ASME CODE STAMPED for __________ PSIG
Receiver: _______ " Diameter x _______ " Long
Automatic Aftercooler Size __________ " sized for __________°F cooling water