FORM SPEC HFT & VFT	COPYRIGHT © 2022 SHIPPENSBURG PUMP COMPANY, INC. 
SHIPCO® IS A REGISTERED TRADEMARK OF SHIPPENSBURG PUMP CO., INC. 	PRINTED IN THE U.S.A. • BEIDEL PRINTING HOUSE, INC., 717-532-5063
SHIPPENSBURG PUMP COMPANY, INC., P.O. BOX 279, SHIPPENSBURG, PA 17257
PHONE 717-532-7321 • FAX 717-532-7704 • www.shipcopumps.com
SuGGESTED SPECIFICATIONS	SHIPCO® PUMPS
TYPE HFT HORIZONTAL FLASH TANK AND
TYPE VFT VERTICAL FLASH TANK
CAPACITY SCHEDULE MUST BE COMPLETED SEPARATELY.

Furnish and install according to drawings and manufacturer’s instructions the quantity of HFT horizontal flash tanks and/or VFT vertical flash tanks as shown on the drawings. Each unit shall consist of (1) ASME code Sec. VIII “U” stamped vessel.
The body shall be made of carbon steel material.
The unit shall be factory tested as a complete unit. The pump manufacturer shall furnish complete elementary piping diagrams, and installation and operation instructions.
Manufacturer shall be Shipco® PUMPS, P.O. Box 279, Shippensburg, PA 17257.
Capacity Schedule (Required to complete suggested specifications).
TYPE HFT & VFT FLASH TANK SCHEDULE:
The Horizontal or Vertical flash tank shall be a carbon steel ASME code Sec. VIII “U” stamped vessel rated for ______ psig maximum vessel pressure. 
ASME code carbon steel flash tank shall measure ______ " x ______ " shell length and have a maximum overall height of ______ " if legs are provided. 
Connections sizes and locations shall be as shown on drawing.
Manufacturer’s standard painting will apply.